Author: Bill Brecks

Install and maintain rock entry/exit way to avoid tracking sediment off the lot.

Trackout due to no rocked exit way. If no exit is available have a plan to return topsoil to lot.

Install and maintain proper silt fencing and catch rolls to ensure sediment doesn’t leave the lot.

Disturbed topsoil near ditch line. Not silt fenced to avoid loss of soil.

Upon completion of job, ensure the lot is covered with natural vegetation to avoid erosion.

Use a concrete washout station to make sure harmful slurry doesn’t enter the waterways.